**Water Filter Test Results**

 All the filters were tested using the same laboratory protocol and ICP-MS instrumentation, all on the same day.

|  |  |  |
| --- | --- | --- |
|    |    | Percent REMOVAL of elements from tested water filters  |
|   |   | **Aluminum** | **Copper** | **Arsenic** | **Strontium** | **Cadmium** | **Cesium** | **Mercury** | **Lead** | **Uranium**  |
| http://labs.naturalnews.com/Photos/100/Water-Filter-ZeroWater.jpg | **ZeroWater**  | 100% | 99.1% | 99.3% | 100% | 99.2% | 100% | 99.4% | 99.2% | 99.1% |
| http://labs.naturalnews.com/Photos/100/Water-Filter-Waterman-Portable.jpg | **WaterMan** | 62.4% | 89.2% | 54.0% | -179.0% | 49.1% | 25.7% | 99.7% | 93.7% | 72.4% |
| http://labs.naturalnews.com/Photos/100/Water-Filter-Pur.jpg | **Pur**  | **-46.8%** | 27.6% | 19.8% | 15.4% | 17.4% | 27.8% | 98.9% | 34.9% | 31.5% |
| http://labs.naturalnews.com/Photos/100/Water-Filter-Seychelle.jpg | **Seychelle**  | **-27.9%** | 39.9% | 78.4% | 30.2% | 27.8% | 38.7% | 99.6% | 72.0% | 43.2% |
| http://labs.naturalnews.com/Photos/100/Water-Filter-Culligan.jpg | **Culligan**  | **-52.4%** | 30.8% | 16.0% | 27.8% | 22.6% | 30.4% | 62.4% | 30.2% | 28.6% |
| http://labs.naturalnews.com/Photos/100/Water-Filter-Mavea.jpg | **Mavea** | 8.1% | 18.8% | 18.6% | 2.4% | 9.2% | 15.3% | 85.0% | 23.4% | 22.7% |
| http://labs.naturalnews.com/Photos/100/Water-Filter-Brita.jpg | **Brita**  | **-33.9%** | 8.6% | 12.1% | 3.6% | 6.6% | 9.5% | 74.6% | 14.1% | 10.0% |

 Minus sign signifies an INCREASE in the element rather than a decrease!!